|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Pay Item** | **Description** | **Qty** | **Unit** | **Unit Price** | **Total Price** |
| 1 | Mobilization | 1 | LS |  |   |
| 2 | Traffic Control | 1 | LS |  |   |
| 3 | Mud Mats | 375 | SY |  |   |
| 4 | Mulch Complete | 650 | SY |  |   |
| 5 | Sodding and Permanent Seeding Complete | 650 | SY |  |  |
| 6 | Temporary Seeding Complete | 650 | SY |  |   |
| 7 | Silt Fence Complete, Type C | 525 | LF |  |   |
| 8 | Compost Filter Sock | 500 | LF |  |  |
| 9 | Tree Protection Fence Complete | 100 | LF |  |  |
| 10 | Construction Entrance Complete | 1 | EA |  |  |
| 11 | Cured In Place Pipe Rehabilitation, 30-IN CMP | 170 | LF |  |  |
| 12 | Flowable Fill | 10 | CY |  |  |
| 13 | Control of Water | 1 | LS |  |  |
| 14 | Sidewalk Replacement | 25 | SY |  |  |
| 15 | W-Beam Guardrail | 55 | LF |  |  |
| 16 | Rip Rap, Type 3, 24-IN Thickness | 65 | SY |  |  |
| 17 | Riser Modifications | 1 | LS |  |   |
| 18 | Grading Complete | 1 | LS |  |  |
| 19 | Plastic Filter Fabric | 75 | SY |  |  |
| 20 | Removal of Existing Storm Drain Pipe | 5 | LF |  |  |
| 21 | Hoist Head Complete – Sluice Gate Structure Component System | 1 | EA |  |  |
| 22 | Stem Guides Complete - Sluice Gate Structure Component System | 1 | EA |  |  |
| 23 | Pedestal Complete – Sluice Gate Structure Component System  | 1 | EA |  |  |
| 24 | Operating Stem Complete – Sluice Gate Structure Component System | 1 | EA |  |  |
| 25 | Gate Complete – Sluice Gate Structure Component System | 1 | EA |  |  |
| 26 | Allowance – Repair/Remove/Lower Abandoned Standpipe | 1 | LS |  |  |
|   | **Low Water Drain CIPP Rehabilitation** | **Total Bid Price** |  |

\*\*\* Include completed bid schedule with your bid.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Pay Item** | **Description** | **Qty** | **Unit** | **Unit Price** | **Total Price** |
| 100 | Install, Maintain, and Remove Special Construction Exit / Lake Access – off Parking Lot | 1 | LS |  |   |
| 200 | Remove All Trees within 3 feet of Spillway, Sheet C-001 | 1 | LS |  |  |
| 300 | Remove All Vegetation on Upstream Slope, Sheet C-001 | 1 | LS |  |  |
| 400 | Replace Missing Animal Guards on Toe Drain Outfalls, Sheet C-001 | 3 | EA |  |   |
| 500 | Remove Tree on Dam | 1 | EA |  |   |
| 600 | Make Designated Repairs, NE Side of Spillway, Sheet C-002 | 1 | LS |  |   |
| 700 | Remove All Vegetation On and Around Spillway Masonry Wall and Repair Wall Grout, Seal Transverse Joints, Sheet C-002 | 1 | LS |  |  |
| 800 | Repair and Seal Joints on Spillway / Repair Broken Concrete, Sheet C-002 | 1 | LS |  |  |
| 900 | Rip Rap | 400 | TN |  |   |
| 1000 | Install and Maintain Orange Tree Barrier Fencing Around Work Areas | 1 | LS |  |  |
| 1100 | Double Row Type C Silt Fence | 100 | LF |  |   |
|   | **Dam & Spillway Maintenance / Repairs Bid** | **Total Bid Price** |  |

\*\*\* Include completed bid schedule with your bid

**THE PROJECT SCOPE OF WORK IS FOR ALL WORK LISTED.**

**CONTRACTOR MUST COMPLETE BOTH BID FORMS TO BE CONSIDERED RESPONSTIVE**

**Total Bid Amount:**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Total Bid Amount:**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Contractor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Signature:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Print:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Date:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**THIS PAGE MUST BE COMPLETED AND SUBMITTED AS A PART OF YOUR BID**

***\*\*\*\*\*\*END OF EXHIBIT K\*\*\*\*\****